**FURNITURE & ACCESSORIES**

**BASE & WALL UNITS**

**To Medical Areas**

Base and wall units to all clinical areas i.e. Treatment & utility rooms to be HTM63 compliant. (noted as 'HTM compliant room' under special comments section on room data sheets)

**Manufacturer and reference:**

David Bailey Furniture Systems

Tel: 01843 604896

Email: sales@davidbaileyfurniture.co.uk

12 Lysander Close, Pysons Road Industrial Estate, Broadstairs, Kent CT10 2YJ

**Carcass**: 18mm thick 750 Kg/m3 MFC fully assembled internally doweled and glued. Finished in white 120g melamine with 1mm pvc tape to all edges. All base units have 12mm white melamine faced MFC backs. Sink units supplied with backs removable from interior. 100mm void as standard. Includes 1 shelf unit as standard, finished in white melamine MFC

**Door & Drawer**: 18mm thick 750kg/m3 MDF finished in colour from Polyrey Collection with 2mm pvc tape to edges.

**Drawer Boxes**: White enamel ‘Blum’ Metabox system, with power coated metal drawer runners with nylon rollers, 12mm white MFC base and 18mm backs.

**Plinths**: Where required 18mm black melamine faced MDF board fixed via clips to adjustable feet.

**Hinges**: 170 degree, fully concealed sprung ‘Blum’

**Locks**: ‘Hafele’ Symo 3000 cylinder lock.

**Handles**: 96 x 10mm 'D' type

**DRAWER BOXES**

Units to have matching end panels to walls & base units as necessary

**WORKTOPS**

Worktops to all clinical areas to be HTM63 compliant as below:

To include all necessary support legs

**Worktops**: Ref: HTM63, 600mm deep, 40mm thick post formed laminate bullnose to front edge and integral 50mm high integral rear upstand.

**Worktops to desk areas:**

750mm deep, 40mm thick single Bullnosed high pressure laminated worktop, Polyrey laminate or equal approved.

Support legs as necessary, 30mm dia. tubular steel leg white finish or equal approved.

All worktops to receive laminate edging to exposed ends.